**BC-221 Output Information**

Output is -17 dbm or 18 microwatts, which is 17 db below 1 milliwatt.

Output is about 0.7 volt Peak-to-Peak into a 50 ohm load.

Output measures 3 volts with no load